|  |  |
| --- | --- |
| Proposed Start & End Time: |  |
| Contractor: |  |
| Description of Work: |  |
| Competent Person: |  |
| Work Location: |  |

Type of Work Performed (select all that apply):

* Cutting
* Soldering / Grinding
* Oxy / Acetylene Torch
* Gas Welding
* Electric Arc Welding
* Acetylene / MAPP Gas

Required Precautions (check all that apply):

General:

* Cutting and welding equipment in good condition
* Sprinkler system in service
* Fire Extinguisher in good condition and available

Requirements within 35 Feet of Work:

* Floors swept and clean of combustible material
* Combustible floors (e.g. wood, tile, carpet, etc.) wet down, covered with damp sand or fire blankets
* No flammable materials stored in area
* Wall and floor openings covered
* Walkways protected beneath hot work

Work on Wall or Ceiling:

* Combustibles removed from other side of wall
* Construction is non-combustible and without combustible covering or insulation

Work in Confined Space:

* Confined Space Permit
* Equipment cleaned of all liquid combustibles
* Containers purged of vapors

Fire Watch:

* Fire watch will be provided during and for 30 minutes after work (including breaks)
* Fire watch is supplied with and extinguisher and/or water pump can
* Fire watch is trained on use of equipment

|  |  |
| --- | --- |
| **Authorized Personnel:** | |
| **Role:** | **Name:** |
| Fire Watch |  |
| Welder |  |
| Supervisor |  |
| Other |  |

|  |  |
| --- | --- |
| **Signatures:** | |
| Contractor Supervisor: |  |
| Fire Watch: |  |